**SEED SOWING MACHINE**

In this seed sowing process to avoid the drawbacks. The seed sowing machine is developed which has very less cost. Also the unskilled farmer can be easily operated automatic seed sowing system. In this design, the drive shaft directly controls the seed metering mechanism which eliminates completely attachments such as pulleys, belts system, thereby eliminating complexities which increase the cost, and increasing efficiency at a highly reduced cost which is the focus of this project work. This system is very much beneficial to all farmers because the wastage of seeds and more man power are avoided for that system. Also the time to be saves. All facilities to be provided in automatic seed sowing machine. This system provides to all the facility which can work efficiently. Also the farmer can sow the seed very much easily. As well as time will be save. This system is very useable to farmer, seed can be sow automatically.

It can do three tasks together. Digging, sowing, and refilling the sand. Generally these are done

using three different machines.

Its cost is also less compared to the other machines available in the market.

It does not require any electricity to run the machine.

 